SOP Steps for backup Vlan ip config---

1. Change in the ip of main interface(Comment# the gateway ip) & uncomment the 2nd ip-ens224.

2. Ping the Gateway ip

3. restart(reset) the sever from vCenter.

**Raise Below ITSSP request-**

DNS Services - Modify A-record

DNS Services - New CNAME

DNS Services - New A-record -- Vxlan Ip we have to Put

Format

VXLAN IP - 10.97.205.198

VXLAN DNS - is-voe45ma01d.oneadr.net

VLAN IP -10.97.212.6

VLAN DNS -is-voe45ma01d-vir.oneadr.net