We have to Follow Below Steps:

Before this Activity begins wintel team have to make Change Request.

1. First, we have to take VLAN from Manoj Sinha {By BAU NSX team}.
2. Unix team have to take console from Vmware.
3. Then vmware team have to change that VLAN from Old to new.
4. Then server will be not reachable, Unix team have to restart the network from console, and server will take new Ip after Network restart.
5. Then Unix team have to resolve DNS from new ip by raising ITSSP {for forward and reverse Lookup}